(module BatteryHolder_Keystone_1058_1x2032 (layer F.Cu) (tedit 589EE147)
  (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
  (tags "Keystone type 1058 coin cell retainer")
  (attr smd)
  (fp_text reference REF** (at 0 7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BatteryHolder_Keystone_1058_1x2032 (at 0 -9.398) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 0 0) (end 11.06 4.11) (angle 139.2) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end -11.06 -4.11) (angle 139.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.06 4.11) (end 16.45 4.11) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.45 4.11) (end 16.45 -4.11) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.45 -4.11) (end 11.06 -4.11) (layer F.CrtYd) (width 0.05))
  (fp_line (start -16.45 -4.11) (end -11.06 -4.11) (layer F.CrtYd) (width 0.05))
  (fp_line (start -16.45 -4.11) (end -16.45 4.11) (layer F.CrtYd) (width 0.05))
  (fp_line (start -16.45 4.11) (end -11.06 4.11) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end -10.692 3.61) (angle -27.3) (layer F.SilkS) (width 0.12))
  (fp_arc (start 0 0) (end 10.692 -3.61) (angle -27.3) (layer F.SilkS) (width 0.12))
  (fp_arc (start 0 0) (end 10.692 3.61) (angle 27.3) (layer F.SilkS) (width 0.12))
  (fp_arc (start 0 0) (end -10.692 -3.61) (angle 27.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.31 1.9) (end -14.31 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.692 3.61) (end -14.31 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.86 8.11) (end -7.8473 8.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.66 5.91) (end -3.86 8.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 5.91) (end -1.66 5.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.66 5.91) (end 3.86 8.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.8473 8.11) (end 3.86 8.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.31 1.9) (end 14.31 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.31 3.61) (end 10.692 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.692 -3.61) (end 14.31 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.31 -1.9) (end 14.31 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.8473 -8.11) (end 7.8473 -8.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.31 -1.9) (end -14.31 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.31 -3.61) (end -10.692 -3.61) (layer F.SilkS) (width 0.12))
  (fp_arc (start 0 0) (end -10.61275 3.5) (angle -27.4635) (layer F.Fab) (width 0.1))
  (fp_arc (start 0 0) (end 10.61275 -3.5) (angle -27.4635) (layer F.Fab) (width 0.1))
  (fp_arc (start 0 0) (end 10.61275 3.5) (angle 27.4635) (layer F.Fab) (width 0.1))
  (fp_line (start 14.2 1.9) (end 14.2 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 14.2 3.5) (end 10.61275 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 10.61275 -3.5) (end 14.2 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 14.2 -3.5) (end 14.2 -1.9) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 1.9) (end -14.2 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 3.5) (end -10.61275 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.9 8) (end 7.8026 8) (layer F.Fab) (width 0.1))
  (fp_line (start 1.7 5.8) (end 3.9 8) (layer F.Fab) (width 0.1))
  (fp_line (start -1.7 5.8) (end -3.9 8) (layer F.Fab) (width 0.1))
  (fp_line (start -1.7 5.8) (end 1.7 5.8) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 -3.5) (end -10.61275 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 -3.5) (end -14.2 -1.9) (layer F.Fab) (width 0.1))
  (fp_line (start -3.9 8) (end -7.8026 8) (layer F.Fab) (width 0.1))
  (fp_line (start -7.8026 -8) (end 7.8026 -8) (layer F.Fab) (width 0.1))
  (fp_arc (start 0 0) (end -10.61275 -3.5) (angle 27.4635) (layer F.Fab) (width 0.1))
  (fp_circle (center 0 0) (end 10 0) (layer Dwgs.User) (width 0.15))
  (pad 1 smd rect (at -14.68 0) (size 2.54 3.51) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 14.68 0) (size 2.54 3.51) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1058_1x2032.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
