(module BatteryHolder_Keystone_1060_1x2032 (layer F.Cu) (tedit 5B98EF5E)
  (descr http://www.keyelco.com/product-pdf.cfm?p=726)
  (tags "CR2032 BR2032 BatteryHolder Battery")
  (attr smd)
  (fp_text reference REF** (at -14.125 -5.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BatteryHolder_Keystone_1060_1x2032 (at 0 -11.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end -10.2 0) (layer Dwgs.User) (width 0.3))
  (fp_line (start 11 8) (end -9.4 8) (layer F.Fab) (width 0.1))
  (fp_line (start 11 -8) (end -11 -8) (layer F.Fab) (width 0.1))
  (fp_line (start 11 8) (end 11 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 11 -8) (end 11 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -11 -8) (end -11 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -11 6.4) (end -11 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -11 3.5) (end -14.2 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 3.5) (end -14.2 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -14.2 -3.5) (end -11 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 11 3.5) (end 14.2 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 14.2 3.5) (end 14.2 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 14.2 -3.5) (end 11 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -9.4 8) (end -11 6.4) (layer F.Fab) (width 0.1))
  (fp_line (start 11.35 3.85) (end 14.55 3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.55 3.85) (end 14.55 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.35 8.35) (end 11.35 3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.35 8.35) (end -9.55 8.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.35 6.55) (end -11.35 3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.55 8.35) (end -11.35 6.55) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.35 3.85) (end -14.55 3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.55 3.85) (end -14.55 2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.35 -3.85) (end -14.55 -3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.55 -3.85) (end -14.55 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.35 -3.85) (end 14.55 -3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.55 -3.85) (end 14.55 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.35 -8.35) (end 11.35 -8.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.35 -8.35) (end -11.35 -3.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.35 -8.35) (end 11.35 -3.85) (layer F.SilkS) (width 0.12))
  (fp_arc (start 0 0) (end -6.5 8.5) (angle -74.81070976) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.5 8.5) (end 6.5 8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.5 8.5) (end -11.5 8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.5 4) (end -11.5 8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 4) (end -11.5 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 4) (end -14.7 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 2.3) (end -16.45 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -16.45 2.3) (end -16.45 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 -2.3) (end -16.45 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 -2.3) (end -14.7 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.7 -4) (end -11.5 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.5 -4) (end -11.5 -8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.5 -8.5) (end -6.5 -8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.5 -8.5) (end 11.5 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.5 -4) (end 14.7 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.7 -4) (end 14.7 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.7 -2.3) (end 16.45 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.45 -2.3) (end 16.45 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.45 2.3) (end 14.7 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.7 2.3) (end 14.7 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.7 4) (end 11.5 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.5 4) (end 11.5 8.5) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end 6.5 -8.5) (angle -74.81070976) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.5 -8.5) (end 6.5 -8.5) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13 5) (end -13 7) (layer F.SilkS) (width 0.12))
  (fp_line (start -12 6) (end -14 6) (layer F.SilkS) (width 0.12))
  (pad 2 smd rect (at 14.65 0 180) (size 2.6 3.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -14.65 0 180) (size 2.6 3.6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1060_1x2032.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
