(export (version D)
  (design
    (source /Users/rbaron/dev/parasite/electronics/parasite/parasite.sch)
    (date "2021 February 23, Tuesday 21:34:19")
    (tool "Eeschema (5.1.2-1)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title parasite52832)
        (company)
        (rev 1.0.0)
        (date 2021-02-23)
        (source parasite.sch)
        (comment (number 1) (value rbaron.net))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600E0E7A))
    (comp (ref D1)
      (value LL4148)
      (footprint Diode_SMD:D_MiniMELF)
      (datasheet http://www.vishay.com/docs/85557/ll4148.pdf)
      (libsource (lib Diode) (part LL4148) (description "100V 0.15A standard switching diode, MiniMELF"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600E601E))
    (comp (ref C1)
      (value 1n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600E6E5B))
    (comp (ref R6)
      (value 1M)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600E7750))
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600FFF47))
    (comp (ref R3)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 601057D9))
    (comp (ref R5)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 601113E2))
    (comp (ref C6)
      (value 100p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 600D105B))
    (comp (ref TP3)
      (value Csen+)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6014264C))
    (comp (ref TP4)
      (value Vsen_out)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60145A9D))
    (comp (ref Cpara1)
      (value 5p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6016579E))
    (comp (ref Q1)
      (value MMBT3904)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (libsource (lib Transistor_BJT) (part MMBT3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60188253))
    (comp (ref Q2)
      (value MMBT3904)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (libsource (lib Transistor_BJT) (part MMBT3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 601897A7))
    (comp (ref U1)
      (value E73-2G4M04S1B)
      (footprint XCVR_E73-2G4M04S1B)
      (fields
        (field (name MANUFACTURER) EBYTE)
        (field (name MAXIMUM_PACKAGE_HEIGHT) 2.7mm)
        (field (name PARTREV) 1.4)
        (field (name STANDARD) "Manufacturer Recommendations"))
      (libsource (lib E73-2G4M04S1B) (part E73-2G4M04S1B) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60359A82))
    (comp (ref TP2)
      (value CLK)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6035D56E))
    (comp (ref TP1)
      (value IO)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6035E763))
    (comp (ref TP7)
      (value VCC)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6037D82C))
    (comp (ref TP6)
      (value GND)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6037E819))
    (comp (ref R2)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6037FE48))
    (comp (ref D2)
      (value LED)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6038131F))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint kicad:BatteryHolder_Keystone_3002_1x2032)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60386A6F))
    (comp (ref Q3)
      (value AO3407A)
      (footprint SOT95P280X125-3N)
      (fields
        (field (name MANUFACTURER) "Alpha and Omega Semiconductor")
        (field (name PARTREV) 5)
        (field (name STANDARD) IPC-7351B))
      (libsource (lib AO3407A) (part AO3407A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60388E46))
    (comp (ref JP1)
      (value Jumper)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60392DA9))
    (comp (ref TP5)
      (value RST)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039FE47))
    (comp (ref U2)
      (value SHT30-DIS-B)
      (footprint DFN250X250X100-9N)
      (fields
        (field (name MANUFACTURER) Sensirion))
      (libsource (lib SHT30-DIS-B) (part SHT30-DIS-B) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 603581DD))
    (comp (ref C2)
      (value 1n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6036F153))
    (comp (ref R8)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60372D0F))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small_US) (description "Resistor, small US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6037481E)))
  (libparts
    (libpart (lib AO3407A) (part AO3407A)
      (fields
        (field (name Reference) Q)
        (field (name Value) AO3407A)
        (field (name Footprint) SOT95P280X125-3N)
        (field (name STANDARD) IPC-7351B)
        (field (name PARTREV) 5)
        (field (name MANUFACTURER) "Alpha and Omega Semiconductor"))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type power_out))
        (pin (num 2) (name -) (type power_out))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Jumper)
      (description "Jumper, normally closed")
      (docs ~)
      (footprints
        (fp SolderJumper*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R_Small_US)
      (description "Resistor, small US symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small_US))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Diode) (part LL4148)
      (aliases
        (alias LL4448))
      (description "100V 0.15A standard switching diode, MiniMELF")
      (docs http://www.vishay.com/docs/85557/ll4148.pdf)
      (footprints
        (fp D*MiniMELF*))
      (fields
        (field (name Reference) D)
        (field (name Value) LL4148)
        (field (name Footprint) Diode_SMD:D_MiniMELF))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib E73-2G4M04S1B) (part E73-2G4M04S1B)
      (fields
        (field (name Reference) U)
        (field (name Value) E73-2G4M04S1B)
        (field (name Footprint) XCVR_E73-2G4M04S1B)
        (field (name PARTREV) 1.4)
        (field (name MANUFACTURER) EBYTE)
        (field (name STANDARD) "Manufacturer Recommendations")
        (field (name MAXIMUM_PACKAGE_HEIGHT) 2.7mm))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name DEC2) (type BiDi))
        (pin (num 4) (name DEC3) (type BiDi))
        (pin (num 5) (name P0.25) (type BiDi))
        (pin (num 6) (name P0.26) (type BiDi))
        (pin (num 7) (name P0.27) (type BiDi))
        (pin (num 8) (name P0.28) (type BiDi))
        (pin (num 9) (name P0.29) (type BiDi))
        (pin (num 10) (name P0.30) (type BiDi))
        (pin (num 11) (name P0.31) (type BiDi))
        (pin (num 12) (name DEC4) (type BiDi))
        (pin (num 13) (name DCC) (type output))
        (pin (num 14) (name DEC1) (type BiDi))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VCC) (type power_in))
        (pin (num 17) (name P0.02) (type BiDi))
        (pin (num 18) (name P0.03) (type BiDi))
        (pin (num 19) (name P0.04) (type BiDi))
        (pin (num 20) (name P0.05) (type BiDi))
        (pin (num 21) (name P0.06) (type BiDi))
        (pin (num 22) (name P0.07) (type BiDi))
        (pin (num 23) (name P0.08) (type BiDi))
        (pin (num 24) (name P0.09) (type BiDi))
        (pin (num 25) (name P0.10) (type BiDi))
        (pin (num 26) (name P0.11) (type BiDi))
        (pin (num 27) (name P0.12) (type BiDi))
        (pin (num 28) (name P0.13) (type BiDi))
        (pin (num 29) (name P0.14) (type BiDi))
        (pin (num 30) (name P0.15) (type BiDi))
        (pin (num 31) (name P0.16) (type BiDi))
        (pin (num 32) (name P0.17) (type BiDi))
        (pin (num 33) (name P0.18) (type BiDi))
        (pin (num 34) (name P0.19) (type BiDi))
        (pin (num 35) (name P0.20) (type BiDi))
        (pin (num 36) (name P0.21) (type BiDi))
        (pin (num 37) (name SWDCLK) (type input))
        (pin (num 38) (name SWDIO) (type BiDi))
        (pin (num 39) (name P0.22) (type BiDi))
        (pin (num 40) (name P0.23) (type BiDi))
        (pin (num 41) (name P0.24) (type BiDi))
        (pin (num 42) (name GND) (type power_in))
        (pin (num 43) (name GND) (type power_in))))
    (libpart (lib SHT30-DIS-B) (part SHT30-DIS-B)
      (fields
        (field (name Reference) U)
        (field (name Value) SHT30-DIS-B)
        (field (name Footprint) DFN250X250X100-9N)
        (field (name MANUFACTURER) Sensirion))
      (pins
        (pin (num 1) (name SDA) (type BiDi))
        (pin (num 2) (name ADDR) (type input))
        (pin (num 3) (name ALERT) (type output))
        (pin (num 4) (name SCL) (type BiDi))
        (pin (num 5) (name VDD) (type power_in))
        (pin (num 6) (name ~RESET) (type input))
        (pin (num 7) (name R) (type passive))
        (pin (num 8) (name VSS) (type passive))
        (pin (num 9) (name EXP) (type passive))))
    (libpart (lib Transistor_BJT) (part BC817)
      (aliases
        (alias BC818)
        (alias BC847)
        (alias BC848)
        (alias BC849)
        (alias BC850)
        (alias MMBT3904)
        (alias MMBT5550L)
        (alias MMBT5551L))
      (description "0.8A Ic, 45V Vce, NPN Transistor, SOT-23")
      (docs http://www.fairchildsemi.com/ds/BC/BC817.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC817)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical AO3407A)
      (uri /Users/rbaron/dev/parasite/electronics/lib/snapeda/AO3407A.lib))
    (library (logical Connector)
      (uri "/Library/Application Support/kicad/library/Connector.lib"))
    (library (logical Device)
      (uri "/Library/Application Support/kicad/library/Device.lib"))
    (library (logical Diode)
      (uri "/Library/Application Support/kicad/library/Diode.lib"))
    (library (logical E73-2G4M04S1B)
      (uri /Users/rbaron/dev/parasite/electronics/lib/snapeda/E73-2G4M04S1B.lib))
    (library (logical SHT30-DIS-B)
      (uri /Users/rbaron/dev/parasite/electronics/lib/snapeda/SHT30-DIS-B.lib))
    (library (logical Transistor_BJT)
      (uri "/Library/Application Support/kicad/library/Transistor_BJT.lib")))
  (nets
    (net (code 1) (name /PWM)
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref C6) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 2) (name /Csen+)
      (node (ref R1) (pin 2))
      (node (ref Cpara1) (pin 2))
      (node (ref TP3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 3) (name GND)
      (node (ref C1) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref Q3) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref TP6) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref Cpara1) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref Q1) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U2) (pin 8))
      (node (ref Q2) (pin 2))
      (node (ref U1) (pin 0))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 15))
      (node (ref U1) (pin 42))
      (node (ref U1) (pin 43))
      (node (ref C2) (pin 2)))
    (net (code 4) (name /SENS_OUT)
      (node (ref R6) (pin 1))
      (node (ref U1) (pin 18))
      (node (ref TP4) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 5) (name /FAST_DISCH_EN)
      (node (ref U1) (pin 20))
      (node (ref R3) (pin 1)))
    (net (code 6) (name "Net-(Q1-Pad3)")
      (node (ref Q1) (pin 3))
      (node (ref R3) (pin 2))
      (node (ref Q2) (pin 1)))
    (net (code 7) (name "Net-(Q2-Pad3)")
      (node (ref Q2) (pin 3))
      (node (ref R5) (pin 2)))
    (net (code 8) (name "Net-(C6-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 9) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 10) (name /LED)
      (node (ref U1) (pin 19))
      (node (ref R2) (pin 1)))
    (net (code 11) (name "Net-(U1-Pad21)")
      (node (ref U1) (pin 21)))
    (net (code 12) (name "Net-(U1-Pad22)")
      (node (ref U1) (pin 22)))
    (net (code 13) (name "Net-(U1-Pad23)")
      (node (ref U1) (pin 23)))
    (net (code 14) (name "Net-(U1-Pad24)")
      (node (ref U1) (pin 24)))
    (net (code 15) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 16) (name /SDA)
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 26))
      (node (ref R8) (pin 2)))
    (net (code 17) (name /SCL)
      (node (ref U2) (pin 4))
      (node (ref U1) (pin 27))
      (node (ref R7) (pin 1)))
    (net (code 18) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 19) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 20) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 21) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 22) (name "Net-(U1-Pad32)")
      (node (ref U1) (pin 32)))
    (net (code 23) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 24) (name "Net-(U1-Pad34)")
      (node (ref U1) (pin 34)))
    (net (code 25) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 26) (name "Net-(TP5-Pad1)")
      (node (ref TP5) (pin 1))
      (node (ref U1) (pin 36)))
    (net (code 27) (name "Net-(U1-Pad39)")
      (node (ref U1) (pin 39)))
    (net (code 28) (name "Net-(U1-Pad40)")
      (node (ref U1) (pin 40)))
    (net (code 29) (name "Net-(U1-Pad41)")
      (node (ref U1) (pin 41)))
    (net (code 30) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 31) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 32) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 33) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 34) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 35) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 36) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 37) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 38) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 39) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 40) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 41) (name "Net-(TP2-Pad1)")
      (node (ref U1) (pin 37))
      (node (ref TP2) (pin 1)))
    (net (code 42) (name "Net-(TP1-Pad1)")
      (node (ref TP1) (pin 1))
      (node (ref U1) (pin 38)))
    (net (code 43) (name +3V0)
      (node (ref U2) (pin 5))
      (node (ref JP1) (pin 2))
      (node (ref Q3) (pin 2))
      (node (ref TP7) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref C2) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 44) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 45) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref JP1) (pin 1)))
    (net (code 46) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 47) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))))