(module Battery_Panasonic_CR2032-VS1N_Vertical_CircularHoles (layer F.Cu) (tedit 5C857839)
  (descr "Panasonic CR-2032/VS1N battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D348.PDF")
  (tags "battery CR-2032 coin cell vertical")
  (fp_text reference REF** (at 4.825 -5.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Battery_Panasonic_CR2032-VS1N_Vertical_CircularHoles (at 4.825 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 4.825 -2 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -5.225 -3.95) (end 14.875 -3.95) (layer F.Fab) (width 0.1))
  (fp_line (start 14.875 -3.95) (end 14.875 0.1) (layer F.Fab) (width 0.1))
  (fp_line (start -5.225 -3.95) (end -5.225 0.1) (layer F.Fab) (width 0.1))
  (fp_line (start -5.225 0.1) (end 14.875 0.1) (layer F.Fab) (width 0.1))
  (fp_line (start -5.335 -4.06) (end 9.11 -4.06) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.23 -4.06) (end 14.985 -4.06) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.985 -4.06) (end 14.985 0.21) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.335 -4.06) (end -5.335 0.21) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.335 0.21) (end -1.61 0.21) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.61 0.21) (end 14.985 0.21) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.48 -4.78) (end -5.48 1.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.48 1.45) (end 15.13 1.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.48 -4.78) (end 15.13 -4.78) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.13 -4.78) (end 15.13 1.45) (layer F.CrtYd) (width 0.05))
  (fp_text user + (at -2.2 -0.7) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at 0 0 90) (size 2.7 2.7) (drill 2.12) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 10.17 -3.85) (size 1.6 1.6) (drill 1.09) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Battery.3dshapes/Battery_Panasonic_CR2032-VS1N_Vertical_CircularHoles.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
